|  |
| --- |
| Chubb Exposure Assessment Form Mobilization and Site Work |
|  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | Date of Assessment |       |
|  |  | Completed By |       |

|  |  |
| --- | --- |
| Project |       |
| Contract Number |       |
| Contractor |       |
| Supervisor |       |
| Activity Start Date  |       |
| Expected Completion Date |       |
| No. of Workers  |       |

|  |  |  |  |
| --- | --- | --- | --- |
| Operation | Item # | Exposure | Mitigation / Controls |
| 1. Initial site survey, installation of perimeter fencing and equipment mobilization.
 | 1A | Exposures to toxic plants and dangerous animals. |       |
|  | 1B | Exposures to falls from uneven ground surfaces, slopes, trenches, draining ponds, open below ground structures, cliffs etc.  |       |
|  | 1C | Exposure to overhead and underground utilities. Utility mark out requested and completed according to local municipality requirements. |       |
|  | 1D | Project exposure to theft, trespass, and attractive nuisance. (Crime data and proximity to residential housing and schools). |       |
|  | 1E | Expected Time of Arrival for emergency services in the event they are called to the site. |       |
|  | 1F | Wild-fire potential caused by close contact of brush, debris and materials located on project site with introduced heat sources to include equipment engines, torches, and other tools. |       |
|  | 1G | Insufficient and clearly identified locations of approved fire extinguishers and/or other fire protection. |       |
|  | 1H | Failure to maintain sufficient fire watch during and after the potential for wildfires has stopped. |       |
|  | 1I | Failure to provide workers with required proper PPE to safely perform the work at hand. |       |
|  | 1J | Struck by moving heavy mobile equipment and truck traffic. |       |
|  | 1K | Failure to have JHA completed, approved, and reviewed with crew performing the work. |       |
|  |       |       |       |
|  |       |       |       |
|  |       |       |       |
|  |       |       |       |
|  |       |       |       |
| 1. Clearing, grading and installation of temporary office and yard structures to include temporary utilities.
 | 2A | Wild-fire potential caused by close contact of brush, debris and materials located on project site with introduced heat sources to include equipment engines, torches, and other tools. |       |
|  | 2B | Insufficient and clearly identified locations of approved fire extinguishers and/or other fire protection. |       |
|  | 2C | Insufficient ground stability for equipment and yard storage to include cranes, earthmoving equipment, Conex storage box, porta-johns, and office trailers. |       |
|  | 2D | Exposure to public at project perimeter i.e., sidewalks and public access points. |       |
|  | 2E | Exposure to off-site storage and office locations; theft, trespass, attractive nuisance. |       |
|  | 2F | Exposure to non-construction vehicle traffic at entry and exit points as well as vehicle staging areas. |       |
|  | 2G | Limited worker parking available on-site. |       |
|  | 2H | Struck by moving heavy mobile equipment and truck traffic. |       |
|  | 2I | Failure to have JHA completed, approved, and reviewed with crew performing the work. |       |
|  |       |       |       |
|  |       |       |       |
|  |       |       |       |
|  |       |       |       |
|  |       |       |       |