|  |
| --- |
| Chubb Exposure Assessment Form  Mobilization and Site Work |
|  |

|  |  |  |  |
| --- | --- | --- | --- |
|  |  | Date of Assessment |  |
|  |  | Completed By |  |

|  |  |
| --- | --- |
| Project |  |
| Contract Number |  |
| Contractor |  |
| Supervisor |  |
| Activity Start Date |  |
| Expected Completion Date |  |
| No. of Workers |  |

|  |  |  |  |
| --- | --- | --- | --- |
| Operation | Item # | Exposure | Mitigation / Controls |
| 1. Initial site survey, installation of perimeter fencing and equipment mobilization. | 1A | Exposures to toxic plants and dangerous animals. |  |
|  | 1B | Exposures to falls from uneven ground surfaces, slopes, trenches, draining ponds, open below ground structures, cliffs etc. |  |
|  | 1C | Exposure to overhead and underground utilities. Utility mark out requested and completed according to local municipality requirements. |  |
|  | 1D | Project exposure to theft, trespass, and attractive nuisance. (Crime data and proximity to residential housing and schools). |  |
|  | 1E | Expected Time of Arrival for emergency services in the event they are called to the site. |  |
|  | 1F | Wild-fire potential caused by close contact of brush, debris and materials located on project site with introduced heat sources to include equipment engines, torches, and other tools. |  |
|  | 1G | Insufficient and clearly identified locations of approved fire extinguishers and/or other fire protection. |  |
|  | 1H | Failure to maintain sufficient fire watch during and after the potential for wildfires has stopped. |  |
|  | 1I | Failure to provide workers with required proper PPE to safely perform the work at hand. |  |
|  | 1J | Struck by moving heavy mobile equipment and truck traffic. |  |
|  | 1K | Failure to have JHA completed, approved, and reviewed with crew performing the work. |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
| 1. Clearing, grading and installation of temporary office and yard structures to include temporary utilities. | 2A | Wild-fire potential caused by close contact of brush, debris and materials located on project site with introduced heat sources to include equipment engines, torches, and other tools. |  |
|  | 2B | Insufficient and clearly identified locations of approved fire extinguishers and/or other fire protection. |  |
|  | 2C | Insufficient ground stability for equipment and yard storage to include cranes, earthmoving equipment, Conex storage box, porta-johns, and office trailers. |  |
|  | 2D | Exposure to public at project perimeter i.e., sidewalks and public access points. |  |
|  | 2E | Exposure to off-site storage and office locations; theft, trespass, attractive nuisance. |  |
|  | 2F | Exposure to non-construction vehicle traffic at entry and exit points as well as vehicle staging areas. |  |
|  | 2G | Limited worker parking available on-site. |  |
|  | 2H | Struck by moving heavy mobile equipment and truck traffic. |  |
|  | 2I | Failure to have JHA completed, approved, and reviewed with crew performing the work. |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |